**Open CV Challenges**

Task 1 Face Detection:

Make sure the open cv library is installed on your raspberry pi. Use “pip list” or “pip3 list” to check. If it is not installed, run “pip3 install opencv-python” in your terminal.

Next you need to download the trained face classifier from this [website](https://raw.githubusercontent.com/opencv/opencv/master/data/haarcascades/haarcascade_frontalface_default.xml) and then save it to your working directory.



The code above is used to detect faces from images. Note that for the neural network to work, you need to convert your image to grayscale first. Do this in the blank space in the code above.

Task 2 Facial Cropping:

The Task here is to take an image of a face as input, and crop it such that the facial region is only visible. Start off by downloading the facenet-pytorch library. This contains pre trained face detection and recognition models. Use “pip3 install facenet-pytorch” to download the library.

Next, use this code to crop an image containing a face of your choice:



You have two tasks here, the first is to play around with the margin parameter so that you have the least amount of background possible in your cropped image.

Second task is to modify the code so that instead of taking in a pre saved image, it takes in an image you captured directly from your pi cam as input and crops it.

Challenge 1:

Modify the code in task 1 so that instead of taking in a single image as input, it can take a video in instead. Hint: Extract each frame of the video before running your face detector on it. Bonus points if you get it working directly with video from pi cam.

Challenge 2:

Modify the code in task 2 so that it crops a video sequence instead of single images. Bonus points if you have it do it directly using a recording from your pi camera.